- ASUS (some of them)
1. Get administrator password
2. Get LAN configuration without authentication
3. Get wireless settings without authentication

- Alpha Networks (D-Link firmware)
1. Get administrator username and password

- D-Link DAP-1353, DIR-300, DIR-320
1. Authentication bypass
2. Get administrator password

- D-Link DI-524
1. Get administrator password with user privileges

- D-Link DIR-100 (firmware 4.02 and 4.03)
1. Get settings without authentication
2. Get administrator password

- D-Link DIR-615
1. Get administrator password with user privileges

- D-Link DIR-628, D-Link DIR-655
1. MD5+salt authentication
2. Captcha bypass

- D-Link DIR-825
1. Get administrator password with user privileges

- SerComm Beeline Smart Box S1000
1. Get device settings and administrator password

- Tenda 11N
1. Get administrator password

- Ubicom firmware (tested on TRENDnet TEW-631BRP)
1. Get administrator password with user privileges

- Vertex Wireless VW200
1. Get settings without authentication

- ZTE F660, ZXV10 W300, ZXV10 H108L, and other
1. Authentication bypass
2. Get administrator username and password

- ZTE ZXDSL 531BII
1. Get administrator password

- ZTE ZXDSL 831AII
1. Get administrator password

- ZTE ZXDSL 831CII
1. Get administrator password

- ZyWALL / ZyNOS
1. Get administrator password without authentication, or with user privileges (rom-0 configuration file)